;------------------------------------------------------------------------
; BlueletFAXMDM.INF
; IVT Corporation Bluetooth FAX Modem Installation Script
; For Windows98SE/ME/2000/XP
;
; Copyright (c) 2000-2004, IVT Corporation.
; http://www.ivtcorporation.com
; http://www.bluesoleil.com
;
;------------------------------------------------------------------------

[Version]
Signature="$CHICAGO$"
Class=Modem
Provider=%IVT%
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
DriverVer=07/29/2004,1.0.6

[Manufacturer]
%IVT% = IVT

[IVT]
%BlueletModem%  = Modemreg, MDMBTFAX

[Modemreg]
AddReg=All, BTFAXModem, External

[All]
HKR,,ConfigDialog,,modemui.dll
HKR,,DevLoader,,*vcomm
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"
HKR,,FriendlyDriver,,unimodem.vxd
HKR,,PortSubClass,1,02
HKR,,CompatibilityFlags, 1, 01, 00, 00, 00
HKR,,DCB, 1, 1C,00,00,00, 00,C2,01,00, 15,20,00,00, 00,00,0A,00, 0A,00,08,00, 00,11,13,00, 00,00
HKR,, Properties, 1, 00,00,00,00, FF,00,00,00, 00,00,00,00, 07,00,00,00, 07,00,00,00, 00,03,00,00, 00,C2,01,00, 00,F4,01,00

HKR, Init, 1,, "AT<cr>"
HKR, Init, 2,, "AT&FE0V1X0&D2&C1S0=0<cr>"


HKR, Settings, CallSetupFailTimer,, "S7=<#>" 
HKR,,InactivityScale,1,0a,00,00,00

HKR, Monitor, 1,, "ATS0=0<cr>"
HKR, Monitor, 2,, "None"
HKR, Answer, 1,, "ATA<cr>"
HKR, Hangup, 1,, "ATH<cr>"
HKR,, Reset,, "AT&F<cr>"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Terminator,, "<cr>"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, DialSuffix,, ""
HKR, Settings, Blind_Off,, "X3"
HKR, Settings, Blind_On,, "X1"
HKR, Settings, Pulse,, "P"
HKR, Settings, Tone,, "T"
;HKR, Settings, SpeakerVolume_Low,, "L0"
HKR, Settings, SpeakerVolume_Low,, "L1"
HKR, Settings, SpeakerVolume_Med,, "L2"
HKR, Settings, SpeakerVolume_High,, "L3"
HKR, Settings, SpeakerMode_Off,, "M0"
HKR, Settings, SpeakerMode_Dial,, "M1"
HKR, Settings, SpeakerMode_On,, "M2"


;HKR, Responses, "<cr>",     1,01,0,0,0,0,0,0,0,0,0
;HKR, Responses, "<lf>",     1,01,0,0,0,0,0,0,0,0,0
HKR, Responses, "0<cr>",    1,00,0,0,0,0,0,0,0,0,0   ; OK
HKR, Responses, "1<cr>",    1,02,0,0,0,0,0,0,0,0,0   ; CONNECT
HKR, Responses, "2<cr>",    1,08,0,0,0,0,0,0,0,0,0   ; RING
HKR, Responses, "3<cr>",    1,04,0,0,0,0,0,0,0,0,0   ; NO CARRIER
HKR, Responses, "4<cr>",    1,03,0,0,0,0,0,0,0,0,0   ; ERROR
HKR, Responses, "5<cr>",    1,02,0,B0,04,0,0,0,0,0,0 ; CONNECT 1200
HKR, Responses, "6<cr>",    1,05,0,0,0,0,0,0,0,0,0   ; NO DIALTONE
HKR, Responses, "7<cr>",    1,06,0,0,0,0,0,0,0,0,0   ; BUSY
HKR, Responses, "8<cr>",    1,07,0,0,0,0,0,0,0,0,0   ; NO ANSWER
HKR, Responses, "10<cr>", 1, 02, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "11<cr>", 1, 02, 00, c0,12,00,00, 00,00,00,00

HKR, Responses,"<cr><lf>BUSY<cr><lf>",        1,6,0,0,0,0,0,0,0,0,0
HKR, Responses,"<cr><lf>ERROR<cr><lf>",       1,3,0,0,0,0,0,0,0,0,0
HKR, Responses,"<cr><lf>NO ANSWER<cr><lf>",   1,7,0,0,0,0,0,0,0,0,0
HKR, Responses,"<cr><lf>NO CARRIER<cr><lf>",  1,4,0,0,0,0,0,0,0,0,0
HKR, Responses,"<cr><lf>NO DIAL TONE<cr><lf>",1,5,0,0,0,0,0,0,0,0,0
HKR, Responses,"<cr><lf>NO DIALTONE<cr><lf>", 1,5,0,0,0,0,0,0,0,0,0
HKR, Responses,"<cr><lf>OK<cr><lf>",          1,0,0,0,0,0,0,0,0,0,0
HKR, Responses,"<cr><lf>RING<cr><lf>",        1,8,0,0,0,0,0,0,0,0,0
HKR, Responses,"<cr><lf>CONNECT<cr><lf>",1,02,0,00,00,00,00,00,00,00,00


[BTFAXModem]
;HKR,, VoiceProfile, 1, 00,00,00,00
HKR, Fax, HighestSendSpeed,,0
HKR, Fax, LowestSendSpeed,,0
HKR, Fax, EnableV17Send,,1
HKR, Fax, EnableV17Recv,,1
HKR, Fax, FixModemClass,, "1"
HKR, Fax, ResetCommand,, "AT&FS0=0E0V1"
HKR, Fax, SetupCommand,, "AT&D2"

[External]
HKR,,DeviceType,1,01

[Strings]
IVT = "IVT Corporation"
BlueletModem= "Bluetooth Fax Modem"


