# Copyright (c) 2009-2011 Intel Corporation  
# *****************************************************************************************************  
# *****************************************************************************************************  
# **    Filename:  txtsetup.oem  
# **    Revision:  DRIVER_INFO  
# **    Abstract:  Windows* OEM File for Intel(R)Rapid Storage Technology Enterprise RAIDPort SATA Drivers  
# *****************************************************************************************************  
#  
[Disks]  
#  
# This section lists all disks in the disk set.  
#  
# <description> is a descriptive name for a disk, used when  
#   prompting for the disk  
# <tagfile> is a file whose presence allows setup to recognize  
#   that the disk is inserted.  
# <directory> is where the files are located on the disk.  
#  
#  
disk1 = "Intel(R) Rapid Storage Technology Enterprise Driver", iaStorF.sys, \  
#  
#  
[Defaults]  
#  
# This section lists the default selection for each 'required'  
# hardware component.  If a line is not present for a component,  
# the default defaults to the first item in the [<component_name>]  
# section (see below).  
#  
# <component_name> is one of computer, display, keyboard, mouse, scsi  
# <id> is a unique <within the component> string to be associated  
#   with an option.  
#  
SCSI = iaStorA_C600  
#  
[scsi]  
#  
# This section lists the options available for a particular component.  
#  
# <id> is the unique string for the option  
# <description> is a text string, presented to the user in a menu  
# <key_name> gives the name of the key to be created for the component in  
#   HKEY_LOCAL_MACHINE\ControlSet001\Services  
#  
; iaStorA.inf  
iaStorA_C600 = "Intel(R) C600 Series Chipset SATA RAID Controller"  
#  
; iaAHCI.inf  
iaStorA_AC600 = "Intel(R) C600 Series Chipset SATA AHCI Controller"  
#  
; iaStorS.inf  
iaStorS_C600  = "Intel(R) C600 Series Chipset SAS RAID Controller"  
iaStorS_SATA0 = "Intel(R) C600 Series Chipset SAS RAID (SATA mode) Controller"  
#  
[Files.scsi.iaStorA_C600]  
driver = disk1, iaStorA.sys, iaStorA  
driver = disk1, iaStorF.sys, iaStorF  
inf    = disk1, iaStorA.inf  
catalog = disk1, iaStorA.cat  
#  
[Files.scsi.iaStorA_AC600]  
driver = disk1, iaStorA.sys, iaStorA  
driver = disk1, iaStorF.sys, iaStorF  
inf    = disk1, iaAHCI.inf  
catalog = disk1, iaAHCI.cat  
#  
[Files.scsi.iaStorS_C600]  
driver = disk1, iaStorS.sys, iaStorS  
driver = disk1, iaStorF.sys, iaStorF  
inf    = disk1, iaStorS.inf  
catalog = disk1, iaStorS.cat  
#  
[Files.scsi.iaStorS_SATA0]  
driver = disk1, iaStorS.sys, iaStorS  
driver = disk1, iaStorF.sys, iaStorF  
inf    = disk1, iaStorS.inf  
catalog = disk1, iaStorS.cat  
#  
# [HardwareIds.scsi.id]  
# <id> corresponds to an id entry in the HwComponent section.  
# <deviceId> specifies the device id for a mass storage device.  
# <service>  specifies the service to be installed for the device.   
# The service is specified by the file name of its executable image without a .sys extension.  
#  
[HardwareIds.scsi.iaStorA_C600]  
id = "PCI\VEN_8086&DEV_2922", "iaStorA"  
id = "PCI\VEN_8086&DEV_2826", "iaStorA"  
#  
[HardwareIds.scsi.iaStorA_AC600]  
id = "PCI\VEN_8086&DEV_1D02", "iaStorA"  
#  
[HardwareIds.scsi.iaStorS_C600]  
id = "PCI\VEN_8086&DEV_1D60", "iaStorS"  
id = "PCI\VEN_8086&DEV_1D61", "iaStorS"  
id = "PCI\VEN_8086&DEV_1D64", "iaStorS"  
id = "PCI\VEN_8086&DEV_1D65", "iaStorS"  
id = "PCI\VEN_8086&DEV_1D68", "iaStorS"  
id = "PCI\VEN_8086&DEV_1D69", "iaStorS"  
#  
[HardwareIds.scsi.iaStorS_SATA0]  
id = "PCI\VEN_8086&DEV_1D6A", "iaStorS"  
id = "PCI\VEN_8086&DEV_1D6B", "iaStorS"  
#  
# [Config.subkey_name]  
# Specifies the name of a key under the Services\DriverKey tree where Windows places the specified value.   
# <value_name> specifies the name of the value to be set.  
# <value_type> specifies the type of the registry entry.   
# The value_type can be one of the following: REG_DWORD, REG_BINARY, REG_MULTI_SZ  
# <value> specifies the value; its format depends on value_type.  
#  
[Config.iaStorA]  
value = Parameters\PnpInterface,5,REG_DWORD,1  
value = Parameters,BusType,REG_DWORD,8  
value = Parameters\Device,EnableQueryAccessAlignment,REG_DWORD,1  
#  
[Config.iaStorS]  
value = Parameters\PnpInterface,5,REG_DWORD,1  
value = Parameters,BusType,REG_DWORD,A  
value = Parameters\Device,EnableQueryAccessAlignment,REG_DWORD,1  
#  
[Config.iaAHCI]  
value = Parameters\PnpInterface,5,REG_DWORD,1  
value = Parameters,BusType,REG_DWORD,B  
value = Parameters\Device,EnableQueryAccessAlignment,REG_DWORD,1  
