;/*++
;
;Copyright (c) 2003-2004 BROADCOM Inc. All rights reserved.
;
;Module Name:
;
;    bchtsw64.INF
;
;Abstract:
;    INF file for installing BROADCOM miniport device drivers
;
;--*/
;        bchtsw64.inf
; 
;
[Version] 
Signature = "$CHICAGO$" 
Class=SCSIAdapter
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider=%BROADCOM% 
CatalogFile=bchtsw64.cat
DriverVer=04/21/2009,1.1.8070.1

[DestinationDirs] 
Htsata.Files.x86_12 = 12

[SourceDisksNames]
0=%Desc_x860%

[SourceDisksFiles]
bchtsw64.sys=0,

[Manufacturer] 
%BROADCOM%=BROADCOM, ntamd64

[BROADCOM.ntamd64]
%HtsataDesc%=Htsata_Inst,PCI\VEN_1166&DEV_024A

[Htsata_Inst.ntamd64] 
CopyFiles = Htsata.Files.x86_12 

[Htsata_Inst.ntamd64.Services] 
AddService = bchtsw64,0x00000002,Htsata_Service_Instx86,Htsata_EventLog_Inst

[Htsata_Service_Instx86] 
ServiceType = %SERVICE_KERNEL_DRIVER% 
StartType = %SERVICE_BOOT_START% 
ErrorControl = %SERVICE_ERROR_NORMAL% 
ServiceBinary = %12%\bchtsw64.sys 
LoadOrderGroup = "SCSI Storport"
AddReg = pnpsafe_pci_addreg

[Htsata.Files.x86_12] 
bchtsw64.sys

[Htsata_EventLog_Inst] 
AddReg = Htsata_EventLog_Inst_AddReg 
 
[Htsata_EventLog_Inst_AddReg] 
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\iologmsg.dll" 
HKR,,TypesSupported,%REG_DWORD%,7

[pnpsafe_pci_addreg] 
HKR, Parameters\PnpInterface, 5, 0x00010001, 0x00000001 

;BusType setting (default SATA) for HT1000.
HKR,"Parameters", "BusType", %REG_DWORD%, 0x0000000b

;Disable Powerup in Standby 
; 0: Enable the powerup in standby feature
; 1: Disable the powerup in standby feature
; Further, check drive jumper setting, the jumper setting overrides the driver feature
HKR,"Parameters\Device", "DisPwrUpInStandby", %REG_DWORD%, 0x00000001

[Strings] 

;  *******Localizable Strings******* 
BROADCOM= "Broadcom(r) Corporation" 
Desc_x860= "Broadcom Corp SCSIAdapterdrivers"
HtsataDesc= "Broadcom HT1000 SATA Controller(AMD64 Release)" 

;  *******Non Localizable Strings******* 



SERVICE_BOOT_START = 0x0 
SERVICE_SYSTEM_START = 0x1 
SERVICE_AUTO_START = 0x2 
SERVICE_DEMAND_START = 0x3 
SERVICE_DISABLED = 0x4 

SERVICE_KERNEL_DRIVER = 0x1 
SERVICE_ERROR_IGNORE = 0x0 
SERVICE_ERROR_NORMAL = 0x1 
SERVICE_ERROR_SEVERE = 0x2 
SERVICE_ERROR_CRITICAL = 0x3 

REG_EXPAND_SZ = 0x00020000 
REG_DWORD = 0x00010001 
