;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;;
;;  Copyright (c) AVerMedia TECHNOLOGIES, Inc.
;;
;;  Installation file for AVerMedia USB Polaris Series Dummy IR Driver
;;
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;

[Version]
Signature="$Chicago$"
Class=USB
ClassGuid={36fc9e60-c465-11cf-8056-444553540000}
Provider=%AVerMedia%
CatalogFile=AVPolDIR.cat
DriverVer=10/07/2010,10.2.0.46

[SourceDisksNames]
1=%DriverDescription%,,,

[SourceDisksFiles]
AVPolDIR.sys=1
WdfCoInstaller01009.dll=1 ; make sure the number matches with SourceDisksNames

[DestinationDirs]
AVPolDIR.CopyFiles=12

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%AVerMedia%=DeviceList,NTx86,NTx86.6

[DeviceList.NTx86]
%DeviceDescriptionH830%=AVPolFIRx86,USB\VID_07CA&PID_3830&MI_00
%DeviceDescriptionH830%=AVPolFIRx86,USB\VID_07CA&PID_4830&MI_00
%DeviceDescriptionA833%=AVPolFIRx86,USB\VID_07CA&PID_1833&MI_00
%DeviceDescriptionA833%=AVPolFIRx86,USB\VID_07CA&PID_2833&MI_00
%DeviceDescriptionA833%=AVPolFIRx86,USB\VID_07CA&PID_3833&MI_00
%DeviceDescriptionC039%=AVPolFIRx86,USB\VID_07CA&PID_C039&MI_00
%DeviceDescriptionC039%=AVPolFIRx86,USB\VID_07CA&PID_D039&MI_00


[DeviceList.NTx86.6]
%DeviceDescriptionH830%=AVPolFIRx86,USB\VID_07CA&PID_3830&MI_00
%DeviceDescriptionH830%=AVPolFIRx86,USB\VID_07CA&PID_4830&MI_00
%DeviceDescriptionA833%=AVPolFIRx86,USB\VID_07CA&PID_1833&MI_00
%DeviceDescriptionA833%=AVPolFIRx86,USB\VID_07CA&PID_2833&MI_00
%DeviceDescriptionA833%=AVPolFIRx86,USB\VID_07CA&PID_3833&MI_00
%DeviceDescriptionC039%=AVPolFIRx86,USB\VID_07CA&PID_C039&MI_00
%DeviceDescriptionC039%=AVPolFIRx86,USB\VID_07CA&PID_D039&MI_00



[AVPolFIRx86.NT]
AddReg=AVPolFIR.AddReg

[AVPolFIR.AddReg]
HKR,,DevLoader,,*ntkern
HKR,"Parameters","MaximumTransferSize",0x10001,256
HKR,"Parameters","DebugLevel",0x10001,2
HKR,"Parameters","A336DummyEnable",0x10001,1

[AVPolFIRx86.NT.Services]
Addservice=,0x00000002


[AVPolFIR.AddService]
DisplayName=%ServiceDescription%
ServiceType=%SERVICE_KERNEL_DRIVER%
StartType=%SERVICE_DEMAND_START%
ErrorControl=%SERVICE_ERROR_NORMAL%
LoadOrderGroup=Base




[Strings]
AVerMedia="AVerMedia TECHNOLOGIES, Inc."

DriverDescription="AVerMedia USB Polaris Series Dummy IR Driver"

DeviceDescriptionH830="AVerMedia H830 USB Dummy IR Receiver"
DeviceDescriptionA833="AVerMedia A833 USB Dummy IR Receiver"
DeviceDescriptionC039="AVerMedia C039 USB Dummy IR Receiver"

ServiceDescription="AVerMedia USB Polaris Series Dummy IR Service"

SERVICE_KERNEL_DRIVER=1
SERVICE_DEMAND_START=3
SERVICE_ERROR_NORMAL=1
