;
;   SER520.INF (for Windows Vista)
;
;   Copyright (c) 2007, Prolific Technology Inc.


[version]
signature="$CHICAGO$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%PRO%
DriverVer=10/24/2007,3.2.0.11
CatalogFile=ser520.cat


; ================= Device Install section =====================

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%PRO%=PRO,NT,NTAMD64

[SourceDisksFiles]
ser520.sys=1
ser52064.sys=1

[SourceDisksNames]
1=%DISK_NAME%,

[DestinationDirs]
DefaultDestDir  = 12

[PRO.NT]
%DeviceDesc% = ComPort, USB\VID_05A1&PID_3064

[PRO.NTAMD64]
%DeviceDesc% = ComPort, USB\VID_05A1&PID_3064

[ComPort.NT]
CopyFiles=ComPort.NT.Copy
AddReg=ComPort.NT.AddReg

[ComPort.NT.HW]
AddReg=ComPort.HW.AddReg

[ComPort.NT.Services]
AddService = Ser520, 0x00000002, Serial_Service_Inst.NT
AddService = Serenum,,Serenum_Service_Inst

[ComPort.NT.Copy]
ser520.sys

[ComPort.NT.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,ser520.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[ComPort.HW.AddReg]
HKR,,"UpperFilters",0x00010000,"serenum"


[ComPort.NTAMD64]
CopyFiles=ComPort.NTAMD64.Copy
AddReg=ComPort.NTAMD64.AddReg

[ComPort.NTAMD64.HW]
AddReg=ComPort.HW.AddReg

[ComPort.NTAMD64.Services]
AddService = Ser520, 0x00000002, Serial_Service_Inst.NTAMD64
AddService = Serenum,,Serenum_Service_Inst

[ComPort.NTAMD64.Copy]
ser52064.sys

[ComPort.NTAMD64.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,ser52064.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"



[Serial_Service_Inst.NT]
DisplayName    = %Serial.SVCDESC%                            
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\ser520.sys
LoadOrderGroup = Base

[Serial_Service_Inst.NTAMD64]
DisplayName    = %Serial.SVCDESC%                            
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\ser52064.sys
LoadOrderGroup = Base

[Serenum_Service_Inst]
DisplayName    = %Serenum.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\serenum.sys
LoadOrderGroup = PNP Filter


[Strings]
PRO = "Prolific"
DeviceDesc = "USC UF-S520 USB-to-Serial Interface"
Serial.SVCDESC  = "USC UF-S520 USB-to-Serial Interface"
Serenum.SVCDESC = "Serenum Filter Driver"
DISK_NAME = "USB-Serial Cable Diskette"
