; BHTPCR.INF, O2Micro/BHT Integrated MMC/SD Controller INF file
; Copyright (c) 1997-2020 O2Micro/BHT Corp.

[Version]
Signature   = "$Windows NT$"
Class       = SCSIAdapter
ClassGuid   = {4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider    = %BayHubTech%
DriverVer = 07/07/2020,1.1.102.1032
Catalogfile = bhtpcrdr.cat

[SourceDisksNames]
1 = %BHTPCRDR.DriverDisk%

[SourceDisksFiles]
bhtpcrdr.sys = 1
bhtv5Icon.dll = 1
SDPA8220.dll = 1

[DestinationDirs]
DefaultDestDir = 12
Copybhtv5Icon = 11
Copybhtv5Icon_WoW64 = 10, sysWoW64
CopySDPA8220 = 11, SDA
CopySDPA8220_WoW64 = 10, sysWoW64\SDA

[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]
%BayHubTech% = BHTPCRDR,NTamd64,NTx86

[BHTPCRDR.NTx86]
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86, PCI\cc_080500		;Default sdhci
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86, PCI\cc_080501		;Default sdhci

%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_1217, PCI\VEN_1217&DEV_8620     ;Seabird
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_8086, PCI\VEN_8086&DEV_9d2d     ;SKL,KBL
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_8086, PCI\VEN_8086&DEV_5aca     ;APL
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_8086, PCI\VEN_8086&DEV_9df5     ;Intel Coffe Lake
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_1022, PCI\VEN_1022&DEV_7906     ;AMD
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_02f5, PCI\VEN_8086&DEV_02f5     ;HP comet Lake-U
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_34f8, PCI\VEN_8086&DEV_34f8     ;HP IceLake

%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_83d2103c, PCI\VEN_8086&DEV_9d2d&SUBSYS_83d2103c ;idx 1, for HP Chromia 14
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_8416103c, PCI\VEN_8086&DEV_9d2d&SUBSYS_8416103c ;idx 2, for HP Chromia 15
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_9d2d8086, PCI\VEN_8086&DEV_9d2d&SUBSYS_9d2d8086 ;idx 3, for Lenovo Yeti2,Kabylake
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_84d8103c, PCI\VEN_8086&DEV_9d2d&SUBSYS_84d8103c ;idx 4, for HP Rumble KBL and KLB-R project
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_856d103c, PCI\VEN_8086&DEV_9df5&SUBSYS_856d103c ;idx 5, for HP 600series Chromia update
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_8536103c, PCI\VEN_8086&DEV_9df5&SUBSYS_8536103c ;idx 6, for HP 400series update 
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_8537103c, PCI\VEN_8086&DEV_9df5&SUBSYS_8537103c ;idx 7, for HP 400series update 
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_85a5103c, PCI\VEN_8086&DEV_9df5&SUBSYS_85a5103c ;idx 8, for HP 400series update 
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_8538103c, PCI\VEN_8086&DEV_9df5&SUBSYS_8538103c ;idx 9, for HP 400series update 
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_85aa103c, PCI\VEN_8086&DEV_9df5&SUBSYS_85aa103c ;idx 10, for HP 400series update 
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_85e2103c, PCI\VEN_8086&DEV_9df5&SUBSYS_85e2103c ;idx 11, for HP BH28PQ10
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_85e3103c, PCI\VEN_8086&DEV_9df5&SUBSYS_85e3103c ;idx 12, for HP BH28PQ10
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_85e4103c, PCI\VEN_8086&DEV_9df5&SUBSYS_85e4103c ;idx 13, for HP BH28PQ10
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_85e5103c, PCI\VEN_8086&DEV_9df5&SUBSYS_85e5103c ;idx 14, for HP BH28PQ10
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_85a3103c, PCI\VEN_8086&DEV_9df5&SUBSYS_85a3103c ;idx 15, for HP 400series update 
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_8649103c, PCI\VEN_8086&DEV_9df5&SUBSYS_8649103c ;idx 16, for HP BH28PQ10
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86ad103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86ad103c ;idx 17, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86ad103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86ad103c ;idx 18, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86ae103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86ae103c ;idx 19, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86ae103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86ae103c ;idx 20, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86af103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86af103c ;idx 21, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86af103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86af103c ;idx 22, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86b0103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86b0103c ;idx 23, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86b0103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86b0103c ;idx 24, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_869b103c, PCI\VEN_8086&DEV_9df5&SUBSYS_869b103c ;idx 25, for HP 400G7
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_869b103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_869b103c ;idx 26, for HP 400G7 update
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_869d103c, PCI\VEN_8086&DEV_9df5&SUBSYS_869d103c ;idx 27, for HP 400G7
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_869d103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_869d103c ;idx 28, for HP 400G7 update
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86a0103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86a0103c ;idx 29, for HP 400G7
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86a0103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86a0103c ;idx 30, for HP 400G7 update
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86a3103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86a3103c ;idx 31, for HP 400G7
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86a3103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86a3103c ;idx 32, for HP 400G7 update
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86a5103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86a5103c ;idx 33, for HP 400G7
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86a5103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86a5103c ;idx 34, for HP 400G7 update
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86a8103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86a8103c ;idx 35, for HP 400G7
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86a8103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86a8103c ;idx 36, for HP 400G7 update
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86bb103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86bb103c ;idx 37, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86bb103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86bb103c ;idx 38, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86bc103c, PCI\VEN_8086&DEV_34f8&SUBSYS_86bc103c ;idx 39, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86bd103c, PCI\VEN_8086&DEV_34f8&SUBSYS_86bd103c ;idx 40, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_86be103c, PCI\VEN_8086&DEV_34f8&SUBSYS_86be103c ;idx 41, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_874b103c, PCI\VEN_8086&DEV_34f8&SUBSYS_874b103c ;idx 42, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_874c103c, PCI\VEN_8086&DEV_34f8&SUBSYS_874c103c ;idx 43, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_87fb103c, PCI\VEN_8086&DEV_34f8&SUBSYS_87fb103c ;idx 44, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_87fc103c, PCI\VEN_8086&DEV_34f8&SUBSYS_87fc103c ;idx 45, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_856e103c, PCI\VEN_8086&DEV_9df5&SUBSYS_856e103c ;idx 46, for HP Coconut
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_882c103c, PCI\VEN_8086&DEV_02f5&SUBSYS_882c103c ;idx 47, for HP CocoR 
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx86_882d103c, PCI\VEN_8086&DEV_02f5&SUBSYS_882d103c ;idx 48, for HP CoconutR 


[BHTPCRDR.NTamd64]
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64, PCI\cc_080500		;Default sdhci
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64, PCI\cc_080501		;Default sdhci

%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_1217, PCI\VEN_1217&DEV_8620     ;Seabird
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_8086, PCI\VEN_8086&DEV_9d2d     ;SKL,KBL
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_8086, PCI\VEN_8086&DEV_5aca     ;APL
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_8086, PCI\VEN_8086&DEV_9df5     ;Intel Coffe Lake
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_1022, PCI\VEN_1022&DEV_7906     ;AMD
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_02f5, PCI\VEN_8086&DEV_02f5     ;HP comet Lake-U
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_34f8, PCI\VEN_8086&DEV_34f8     ;HP IceLake

%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_83d2103c, PCI\VEN_8086&DEV_9d2d&SUBSYS_83d2103c ;idx 1, for HP Chromia 14
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_8416103c, PCI\VEN_8086&DEV_9d2d&SUBSYS_8416103c ;idx 2, for HP Chromia 15
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_9d2d8086, PCI\VEN_8086&DEV_9d2d&SUBSYS_9d2d8086 ;idx 3, for Lenovo Yeti2,Kabylake
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_84d8103c, PCI\VEN_8086&DEV_9d2d&SUBSYS_84d8103c ;idx 4, for HP Rumble KBL and KLB-R project
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_856d103c, PCI\VEN_8086&DEV_9df5&SUBSYS_856d103c ;idx 5, for HP 600series Chromia update
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_8536103c, PCI\VEN_8086&DEV_9df5&SUBSYS_8536103c ;idx 6, for HP 400series update 
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_8537103c, PCI\VEN_8086&DEV_9df5&SUBSYS_8537103c ;idx 7, for HP 400series update 
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_85a5103c, PCI\VEN_8086&DEV_9df5&SUBSYS_85a5103c ;idx 8, for HP 400series update 
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_8538103c, PCI\VEN_8086&DEV_9df5&SUBSYS_8538103c ;idx 9, for HP 400series update 
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_85aa103c, PCI\VEN_8086&DEV_9df5&SUBSYS_85aa103c ;idx 10, for HP 400series update 
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_85e2103c, PCI\VEN_8086&DEV_9df5&SUBSYS_85e2103c ;idx 11, for HP BH28PQ10
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_85e3103c, PCI\VEN_8086&DEV_9df5&SUBSYS_85e3103c ;idx 12, for HP BH28PQ10
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_85e4103c, PCI\VEN_8086&DEV_9df5&SUBSYS_85e4103c ;idx 13, for HP BH28PQ10
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_85e5103c, PCI\VEN_8086&DEV_9df5&SUBSYS_85e5103c ;idx 14, for HP BH28PQ10
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_85a3103c, PCI\VEN_8086&DEV_9df5&SUBSYS_85a3103c ;idx 15, for HP 400series update 
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_8649103c, PCI\VEN_8086&DEV_9df5&SUBSYS_8649103c ;idx 16, for HP 
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86ad103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86ad103c ;idx 17, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86ad103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86ad103c ;idx 18, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86ae103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86ae103c ;idx 19, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86ae103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86ae103c ;idx 20, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86af103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86af103c ;idx 21, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86af103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86af103c ;idx 22, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86b0103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86b0103c ;idx 23, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86b0103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86b0103c ;idx 24, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_869b103c, PCI\VEN_8086&DEV_9df5&SUBSYS_869b103c ;idx 25, for HP 400G7
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_869b103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_869b103c ;idx 26, for HP 400G7 update
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_869d103c, PCI\VEN_8086&DEV_9df5&SUBSYS_869d103c ;idx 27, for HP 400G7
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_869d103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_869d103c ;idx 28, for HP 400G7 update
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86a0103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86a0103c ;idx 29, for HP 400G7
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86a0103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86a0103c ;idx 30, for HP 400G7 update
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86a3103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86a3103c ;idx 31, for HP 400G7
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86a3103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86a3103c ;idx 32, for HP 400G7 update
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86a5103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86a5103c ;idx 33, for HP 400G7
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86a5103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86a5103c ;idx 34, for HP 400G7 update
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86a8103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86a8103c ;idx 35, for HP 400G7
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86a8103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86a8103c ;idx 36, for HP 400G7 update
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86bb103c, PCI\VEN_8086&DEV_9df5&SUBSYS_86bb103c ;idx 37, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86bb103c_02f5, PCI\VEN_8086&DEV_02f5&SUBSYS_86bb103c ;idx 38, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86bc103c, PCI\VEN_8086&DEV_34f8&SUBSYS_86bc103c ;idx 39, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86bd103c, PCI\VEN_8086&DEV_34f8&SUBSYS_86bd103c ;idx 40, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_86be103c, PCI\VEN_8086&DEV_34f8&SUBSYS_86be103c ;idx 41, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_874b103c, PCI\VEN_8086&DEV_34f8&SUBSYS_874b103c ;idx 42, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_874c103c, PCI\VEN_8086&DEV_34f8&SUBSYS_874c103c ;idx 43, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_87fb103c, PCI\VEN_8086&DEV_34f8&SUBSYS_87fb103c ;idx 44, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_87fc103c, PCI\VEN_8086&DEV_34f8&SUBSYS_87fc103c ;idx 45, for HP Pacific series
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_856e103c, PCI\VEN_8086&DEV_9df5&SUBSYS_856e103c ;idx 46, for HP Coconut
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_882c103c, PCI\VEN_8086&DEV_02f5&SUBSYS_882c103c ;idx 47, for HP CocoR 
%BHTPCRDR.sdhci_DeviceDesc% = DriverInstallx64_882d103c, PCI\VEN_8086&DEV_02f5&SUBSYS_882d103c ;idx 48, for HP CoconutR 


[DriverInstallx86.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86;, EventLogService

[DriverInstallx64.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64;, EventLogService

[DriverServicex64]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = default_cfg_se
AddReg         = default_cfg_sb
AddReg         = default_cfg_fj2
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverServicex86]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = default_cfg_se
AddReg         = default_cfg_sb
AddReg         = default_cfg_fj2
AddReg         = default_cfg_intel
AddReg         = autorun_addreg


;Seabird
[DriverInstallx86_1217.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_1217.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_1217.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_1217;, EventLogService

[DriverServicex86_1217]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 1217_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_1217.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_1217.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_1217.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_1217;, EventLogService

[DriverServicex64_1217]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 1217_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[1217_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x00000000
HKR,"seabird", "max_access_mode", 0x00010001, 0x80000003
HKR,"seabird", "max_power_limit", 0x00010001, 0x80000003
HKR,"seabird", "quick_init_card", 0x00010001, 0x80000000
HKR,"seabird", "tuning_mode", 0x00010001, 0x80000000
HKR,"seabird", "emmc_mode", 0x00010001, 0x00000000
HKR,"seabird", "init_delay", 0x00010001, 0x00000000
HKR,"seabird", "ms_sdio_ctrl", 0x00010001, 0x00000000
HKR,"seabird", "mmc_mode_dis", 0x00010001, 0x80000000
HKR,"seabird", "dma_mode_setting", 0x00010001, 0x80000001
HKR,"seabird", "infinite_trans_setting", 0x00010001, 0x00000000
HKR,"seabird", "sdma_boun_setting", 0x00010001, 0x00000020
HKR,"seabird", "tag_queue_capability", 0x00010001, 0x80010010
HKR,"seabird", "freq_200m", 0x00010001, 0x00070004
HKR,"seabird", "freq_100m", 0x00010001, 0x000b0008
HKR,"seabird", "freq_ddr50m", 0x00010001, 0x000d000d
HKR,"seabird", "freq_ddr50m_ituning", 0x00010001, 0x00110011
HKR,"seabird", "freq_75m", 0x00010001, 0x000c000c
HKR,"seabird", "freq_50m", 0x00010001, 0x000e000e
HKR,"seabird", "freq_25m", 0x00010001, 0x000f000f
HKR,"seabird", "freq_400k", 0x00010001, 0x00100010
HKR,"seabird", "recovery_arg_1", 0x00010001, 0xffff0032
HKR,"seabird", "recovery_arg_2", 0x00010001, 0x00030003
HKR,"seabird", "tuning_timeout", 0x00010001, 0x80000096
HKR,"seabird", "write_data_timeout", 0x00010001, 0x800007d0
HKR,"seabird", "read_data_timeout", 0x00010001, 0x800007d0
HKR,"seabird", "non_data_timeout", 0x00010001, 0x800003e8
HKR,"seabird", "r1b_data_timeout", 0x00010001, 0x80001194
HKR,"seabird", "driver_strength_sel", 0x00010001, 0x00000000
HKR,"seabird", "psd_mode", 0x00010001, 0x80000000
HKR,"seabird", "auto_poweroff_time", 0x00010001, 0x00000000
HKR,"seabird", "level1_window_num_100m", 0x00010001, 0x00000005
HKR,"seabird", "level2_window_num_100m", 0x00010001, 0x00000007
HKR,"seabird", "level3_window_num_100m", 0x00010001, 0x00000009
HKR,"seabird", "ssc_cen_100m", 0x00010001, 0x00000080
HKR,"seabird", "ssc_max1_100m", 0x00010001, 0x00000080
HKR,"seabird", "ssc_min1_100m", 0x00010001, 0x00000080
HKR,"seabird", "ssc_max2_100m", 0x00010001, 0x000000a4
HKR,"seabird", "ssc_min2_100m", 0x00010001, 0x00000000
HKR,"seabird", "ssc_max3_100m", 0x00010001, 0x000000a4
HKR,"seabird", "ssc_min3_100m", 0x00010001, 0x00000000
HKR,"seabird", "level1_window_num_200m", 0x00010001, 0x00000005
HKR,"seabird", "level2_window_num_200m", 0x00010001, 0x00000007
HKR,"seabird", "level3_window_num_200m", 0x00010001, 0x00000009
HKR,"seabird", "ssc_cen_200m", 0x00010001, 0x00000060
HKR,"seabird", "ssc_max1_200m", 0x00010001, 0x00000070
HKR,"seabird", "ssc_min1_200m", 0x00010001, 0x00000050
HKR,"seabird", "ssc_max2_200m", 0x00010001, 0x0000007d
HKR,"seabird", "ssc_min2_200m", 0x00010001, 0x00000040
HKR,"seabird", "ssc_max3_200m", 0x00010001, 0x00000080
HKR,"seabird", "ssc_min3_200m", 0x00010001, 0x00000020
HKR,"seabird", "dll_ctrl", 0x00010001, 0x00000099
HKR,"seabird", "sw_sela_sdr104", 0x00010001, 0x000007ff
HKR,"seabird", "init_delay_before_first_cmd", 0x00010001, 0x00000000
HKR,"seabird", "gg_emulator", 0x00010001, 0x20000000
HKR,"seabird", "sw_selb_offset_adjust", 0x00010001, 0x00000000
HKR,"seabird", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000000
HKR,"seabird", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"seabird", "hw_selb_sdr104", 0x00010001, 0x000005ff
HKR,"seabird", "hw_selb_sdr50", 0x00010001, 0x0000077f
HKR,"seabird", "sw_selb_sdr104", 0x00010001, 0x000007ff
HKR,"seabird", "sw_selb_sdr50", 0x00010001, 0x0000077f
HKR,"seabird", "sw_sela_sdr50", 0x00010001, 0x000007ff
HKR,"seabird", "sw_sela_sdr104_valid_failure_range", 0x00010001, 0x000007ff
HKR,"seabird", "sw_sela_sdr104_failure_history", 0x00010001, 0x000007ff
HKR,"seabird", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"seabird", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"seabird", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"seabird", "gg_sw_def12", 0x00010001, 0x00336200
HKR,"seabird", "gg_sw_def13", 0x00010001, 0x00020006
HKR,"seabird", "gg_sw_def14", 0x00010001, 0x40000400
HKR,"seabird", "gg_sw_def15", 0x00010001, 0x40200310
HKR,"seabird", "gg_sw_def16", 0x00010001, 0x18102077
HKR,"seabird", "gg_sw_def2", 0x00010001, 0x04364022
HKR,"seabird", "gg_sw_def3", 0x00010001, 0x51177472
HKR,"seabird", "gg_sw_def4", 0x00010001, 0x01267750
HKR,"seabird", "gg_sw_def5", 0x00010001, 0x10000076
HKR,"seabird", "gg_sw_def6", 0x00010001, 0x21477532
HKR,"seabird", "gg_sw_def7", 0x00010001, 0x05477570
HKR,"seabird", "gg_sw_def8", 0x00010001, 0x62011071
HKR,"seabird", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"seabird", "driver_item", 0x00010001, 0x8000201a
HKR,"seabird", "output_ctrl", 0x00010001, 0x00000019
HKR,"seabird", "sw_sela_sdr50_failure_history", 0x00010001, 0x00000000
HKR,"seabird", "sw_sela_sdr50_valid_failure_range", 0x00010001, 0x000007ff

HKR,"seabird\dmdn", "0x12", 0x00010001, 0x2c280000
HKR,"seabird\dmdn", "0x4", 0x00010001, 0x25100000
HKR,"seabird\dmdn", "0x8", 0x00010001, 0x25100001
HKR,"seabird\dmdn", "0xe", 0x00010001, 0x25100002
HKR,"seabird\dmdn", "0x10", 0x00010001, 0x251000fa
HKR,"seabird\dmdn", "0xf", 0x00010001, 0x25100004
HKR,"seabird\dmdn", "0x18", 0x00010001, 0x25100008

HKR,"seabird\pcr", "000_p0xe2", 0x00010001, 0xf0003000
HKR,"seabird\pcr", "000_p0xfe", 0x00010001, 0x000f0008
HKR,"seabird\pcr", "000_p0x3e6", 0x00010001, 0x00080008
HKR,"seabird\pcr", "000_p0x300", 0x00010001, 0xf0ff6055


;SKL, KBL, APL, Intel Coffe Lake
[DriverInstallx86_8086.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_8086.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_8086.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_8086;, EventLogService

[DriverServicex86_8086]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 8086_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_8086.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_8086.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_8086.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_8086;, EventLogService

[DriverServicex64_8086]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 8086_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[8086_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000041a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106                  
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000005ff          
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f          
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f             
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400                    

;AMD 
[DriverInstallx86_1022.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_1022.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_1022.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_1022;, EventLogService

[DriverServicex86_1022]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 1022_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_1022.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_1022.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_1022.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_1022;, EventLogService

[DriverServicex64_1022]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 1022_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[1022_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000039
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x80008000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x80008000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x80008000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x80008000
HKR,"sd", "driver_item", 0x00010001, 0x8000201a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def9", 0x00010001, 0x30533106                  
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000005ff          
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f          
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f             
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400 

;HP comet Lake-U 
[DriverInstallx86_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_02f5;, EventLogService

[DriverServicex86_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_02f5;, EventLogService

[DriverServicex64_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[02f5_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000099
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10037513
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18102077   
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80000000
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000 
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000101

;HP IceLake 
[DriverInstallx86_34f8.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_34f8.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_34f8.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_34f8;, EventLogService

[DriverServicex86_34f8]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 34f8_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_34f8.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_34f8.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_34f8.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_34f8;, EventLogService

[DriverServicex64_34f8]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 34f8_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[34f8_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000099
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10037513
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18102077   
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80000000
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000 
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000101

;cfg idx 1 
[DriverInstallx86_83d2103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_83d2103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_83d2103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_83d2103c;, EventLogService

[DriverServicex86_83d2103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 83d2103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_83d2103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_83d2103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_83d2103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_83d2103c;, EventLogService

[DriverServicex64_83d2103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 83d2103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[83d2103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "driver_item", 0x00010001, 0x8000041a   
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711   
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513 
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18102077  
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412    
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400    
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x80008000   
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x80008000    
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80000000


;cfg idx 2 
[DriverInstallx86_8416103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_8416103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_8416103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_8416103c;, EventLogService

[DriverServicex86_8416103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 8416103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_8416103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_8416103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_8416103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_8416103c;, EventLogService

[DriverServicex64_8416103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 8416103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[8416103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "driver_item", 0x00010001, 0x8000041a   
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711   
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513 
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18102077  
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412    
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400    
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x80008000   
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x80008000    
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80000000


;cfg idx 3 
[DriverInstallx86_9d2d8086.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_9d2d8086.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_9d2d8086.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_9d2d8086;, EventLogService

[DriverServicex86_9d2d8086]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 9d2d8086_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_9d2d8086.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_9d2d8086.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_9d2d8086.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_9d2d8086;, EventLogService

[DriverServicex64_9d2d8086]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 9d2d8086_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[9d2d8086_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000041a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106       
HKR,"sd", "gg_sw_def16", 0x00010001, 0x58602077           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x0000067f   
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f      
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f       
HKR,"sd", "sw_sela_sdr50", 0x00010001, 0x000003ff      
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01

;cfg idx 4 
[DriverInstallx86_84d8103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_84d8103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_84d8103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_84d8103c;, EventLogService

[DriverServicex86_84d8103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 84d8103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_84d8103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_84d8103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_84d8103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_84d8103c;, EventLogService

[DriverServicex64_84d8103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 84d8103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[84d8103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "driver_item", 0x00010001, 0x8000041a   
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711   
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513 
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18102077  
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412    
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400    
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x80008000   
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x80008000    
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80000000


;cfg idx 5 
[DriverInstallx86_856d103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_856d103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_856d103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_856d103c;, EventLogService

[DriverServicex86_856d103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 856d103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_856d103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_856d103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_856d103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_856d103c;, EventLogService

[DriverServicex64_856d103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 856d103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[856d103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000099
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000041a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10037513
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106                          
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400   
HKR,"sd", "sw_sela_sdr104", 0x00010001, 0x000007ff
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000003ff
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x000007ef
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x000007ef
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000101
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000101


;cfg idx 6 
[DriverInstallx86_8536103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_8536103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_8536103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_8536103c;, EventLogService

[DriverServicex86_8536103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 8536103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_8536103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_8536103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_8536103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_8536103c;, EventLogService

[DriverServicex64_8536103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 8536103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[8536103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00003155
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18202077  
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x000007bf          
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x000007bf           
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000007df          
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000007df
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "psd_mode", 0x00010001, 0x80000000
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010

;cfg idx 7 
[DriverInstallx86_8537103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_8537103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_8537103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_8537103c;, EventLogService

[DriverServicex86_8537103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 8537103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_8537103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_8537103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_8537103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_8537103c;, EventLogService

[DriverServicex64_8537103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 8537103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[8537103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00003255
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x28202077  
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f          
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x0000077f          
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x0000077f
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "psd_mode", 0x00010001, 0x80000000
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx 8 
[DriverInstallx86_85a5103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_85a5103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_85a5103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_85a5103c;, EventLogService

[DriverServicex86_85a5103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 85a5103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_85a5103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_85a5103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_85a5103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_85a5103c;, EventLogService

[DriverServicex64_85a5103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 85a5103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[85a5103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00003255
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x28202077  
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f          
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x0000077f          
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x0000077f
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "psd_mode", 0x00010001, 0x80000000
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx 9 
[DriverInstallx86_8538103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_8538103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_8538103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_8538103c;, EventLogService

[DriverServicex86_8538103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 8538103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_8538103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_8538103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_8538103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_8538103c;, EventLogService

[DriverServicex64_8538103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 8538103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[8538103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00003055
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x08202077  
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f          
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x0000077f          
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x0000077f 
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "psd_mode", 0x00010001, 0x80000000
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx 10 
[DriverInstallx86_85aa103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_85aa103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_85aa103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_85aa103c;, EventLogService

[DriverServicex86_85aa103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 85aa103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_85aa103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_85aa103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_85aa103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_85aa103c;, EventLogService

[DriverServicex64_85aa103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 85aa103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[85aa103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00003055
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x08202077  
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f          
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x0000077f          
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x0000077f 
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "psd_mode", 0x00010001, 0x80000000
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx 11 
[DriverInstallx86_85e2103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_85e2103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_85e2103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_85e2103c;, EventLogService

[DriverServicex86_85e2103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 85e2103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_85e2103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_85e2103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_85e2103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_85e2103c;, EventLogService

[DriverServicex64_85e2103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 85e2103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[85e2103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000041a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18102077   
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000


;cfg idx 12 
[DriverInstallx86_85e3103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_85e3103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_85e3103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_85e3103c;, EventLogService

[DriverServicex86_85e3103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 85e3103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_85e3103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_85e3103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_85e3103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_85e3103c;, EventLogService

[DriverServicex64_85e3103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 85e3103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[85e3103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000041a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18102077   
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000


;cfg idx 13 
[DriverInstallx86_85e4103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_85e4103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_85e4103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_85e4103c;, EventLogService

[DriverServicex86_85e4103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 85e4103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_85e4103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_85e4103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_85e4103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_85e4103c;, EventLogService

[DriverServicex64_85e4103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 85e4103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[85e4103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000041a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18102077   
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000

;cfg idx 14 
[DriverInstallx86_85e5103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_85e5103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_85e5103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_85e5103c;, EventLogService

[DriverServicex86_85e5103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 85e5103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_85e5103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_85e5103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_85e5103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_85e5103c;, EventLogService

[DriverServicex64_85e5103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 85e5103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[85e5103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000041a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18102077   
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000


;cfg idx 15 
[DriverInstallx86_85a3103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_85a3103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_85a3103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_85a3103c;, EventLogService

[DriverServicex86_85a3103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 85a3103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_85a3103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_85a3103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_85a3103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_85a3103c;, EventLogService

[DriverServicex64_85a3103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 85a3103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[85a3103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00003155
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18202077  
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x000007bf          
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x000007bf           
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000007df          
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000007df
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "psd_mode", 0x00010001, 0x80000000
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx 16
[DriverInstallx86_8649103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_8649103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_8649103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_8649103c;, EventLogService

[DriverServicex86_8649103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 8649103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_8649103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_8649103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_8649103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_8649103c;, EventLogService

[DriverServicex64_8649103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 8649103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[8649103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000041a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18102077   
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000


;cfg idx17
[DriverInstallx86_86ad103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86ad103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86ad103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86ad103c;, EventLogService

[DriverServicex86_86ad103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86ad103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86ad103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86ad103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86ad103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86ad103c;, EventLogService

[DriverServicex64_86ad103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86ad103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86ad103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019

HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000

HKR,"sd", "driver_item", 0x00010001, 0x8000001a

HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711

HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513

HKR,"sd", "gg_sw_def16", 0x00010001, 0x38204077   

HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  

HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  

HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        

HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x000006ff          

HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x000006ff            

HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000003ff           

HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000003ff           

HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a

HKR,"sd", "psd_mode", 0x00010001, 0x80040a01

HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a

HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032

HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000303


;cfg idx18 
[DriverInstallx86_86ad103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86ad103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86ad103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86ad103c_02f5;, EventLogService

[DriverServicex86_86ad103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86ad103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86ad103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86ad103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86ad103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86ad103c_02f5;, EventLogService

[DriverServicex64_86ad103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86ad103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86ad103c_02f5_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019

HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000

HKR,"sd", "driver_item", 0x00010001, 0x8000001a

HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711

HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513

HKR,"sd", "gg_sw_def16", 0x00010001, 0x38204077   

HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  

HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  

HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        

HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x000006ff          

HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x000006ff            

HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000003ff           

HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000003ff           

HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a

HKR,"sd", "psd_mode", 0x00010001, 0x80040a01

HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a

HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032

HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000303


;cfg idx19
[DriverInstallx86_86ae103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86ae103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86ae103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86ae103c;, EventLogService

[DriverServicex86_86ae103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86ae103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86ae103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86ae103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86ae103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86ae103c;, EventLogService

[DriverServicex64_86ae103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86ae103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86ae103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019

HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000

HKR,"sd", "driver_item", 0x00010001, 0x8000001a

HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711

HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513

HKR,"sd", "gg_sw_def16", 0x00010001, 0x38204077   

HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  

HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  

HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        

HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x000006ff          

HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x000006ff            

HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000003ff           

HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000003ff           

HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a

HKR,"sd", "psd_mode", 0x00010001, 0x80040a01

HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a

HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032

HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000303


;cfg idx20 
[DriverInstallx86_86ae103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86ae103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86ae103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86ae103c_02f5;, EventLogService

[DriverServicex86_86ae103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86ae103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86ae103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86ae103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86ae103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86ae103c_02f5;, EventLogService

[DriverServicex64_86ae103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86ae103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86ae103c_02f5_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019

HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000

HKR,"sd", "driver_item", 0x00010001, 0x8000001a

HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711

HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513

HKR,"sd", "gg_sw_def16", 0x00010001, 0x38204077   

HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  

HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  

HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        

HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x000006ff          

HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x000006ff            

HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000003ff           

HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000003ff           

HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a

HKR,"sd", "psd_mode", 0x00010001, 0x80040a01

HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a

HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032

HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000303


;cfg idx 21 
[DriverInstallx86_86af103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86af103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86af103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86af103c;, EventLogService

[DriverServicex86_86af103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86af103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86af103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86af103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86af103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86af103c;, EventLogService

[DriverServicex64_86af103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86af103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86af103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019

HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000

HKR,"sd", "driver_item", 0x00010001, 0x8000001a

HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711

HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513

HKR,"sd", "gg_sw_def16", 0x00010001, 0x48504077   

HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  

HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  

HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        

HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           

HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            

HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000006ff           

HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000006ff           

HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a

HKR,"sd", "psd_mode", 0x00010001, 0x80040a01

HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a

HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032

HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000404

;cfg idx 22 
[DriverInstallx86_86af103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86af103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86af103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86af103c_02f5;, EventLogService

[DriverServicex86_86af103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86af103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86af103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86af103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86af103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86af103c_02f5;, EventLogService

[DriverServicex64_86af103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86af103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86af103c_02f5_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019

HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000

HKR,"sd", "driver_item", 0x00010001, 0x8000001a

HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711

HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513

HKR,"sd", "gg_sw_def16", 0x00010001, 0x48504077   

HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  

HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  

HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        

HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           

HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            

HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000006ff           

HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000006ff           

HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a

HKR,"sd", "psd_mode", 0x00010001, 0x80040a01

HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a

HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032

HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000404


;cfg idx 23
[DriverInstallx86_86b0103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86b0103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86b0103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86b0103c;, EventLogService

[DriverServicex86_86b0103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86b0103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86b0103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86b0103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86b0103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86b0103c;, EventLogService

[DriverServicex64_86b0103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86b0103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86b0103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019

HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000

HKR,"sd", "driver_item", 0x00010001, 0x8000001a

HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711

HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513

HKR,"sd", "gg_sw_def16", 0x00010001, 0x48504077   

HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  

HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  

HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        

HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           

HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            

HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000006ff           

HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000006ff           

HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a

HKR,"sd", "psd_mode", 0x00010001, 0x80040a01

HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a

HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032

HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000404


;cfg idx 24
[DriverInstallx86_86b0103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86b0103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86b0103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86b0103c_02f5;, EventLogService

[DriverServicex86_86b0103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86b0103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86b0103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86b0103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86b0103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86b0103c_02f5;, EventLogService

[DriverServicex64_86b0103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86b0103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86b0103c_02f5_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019

HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000

HKR,"sd", "driver_item", 0x00010001, 0x8000001a

HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711

HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513

HKR,"sd", "gg_sw_def16", 0x00010001, 0x48504077   

HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  

HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  

HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        

HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           

HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            

HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000006ff           

HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000006ff           

HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a

HKR,"sd", "psd_mode", 0x00010001, 0x80040a01

HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a

HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032

HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000404


;cfg idx 25 
[DriverInstallx86_869b103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_869b103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_869b103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_869b103c;, EventLogService

[DriverServicex86_869b103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 869b103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_869b103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_869b103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_869b103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_869b103c;, EventLogService

[DriverServicex64_869b103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 869b103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[869b103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000041a
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18202077   
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000007bf           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000007bf
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80000000
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx26 
[DriverInstallx86_869b103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_869b103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_869b103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_869b103c_02f5;, EventLogService

[DriverServicex86_869b103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 869b103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_869b103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_869b103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_869b103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_869b103c_02f5;, EventLogService

[DriverServicex64_869b103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 869b103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[869b103c_02f5_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00003155
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18202077  
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x000007bf          
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x000007bf           
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000007df          
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000007df
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx 27
[DriverInstallx86_869d103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_869d103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_869d103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_869d103c;, EventLogService

[DriverServicex86_869d103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 869d103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_869d103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_869d103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_869d103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_869d103c;, EventLogService

[DriverServicex64_869d103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 869d103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[869d103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000041a
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x28202077   
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x0000077f
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80000000
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx 28
[DriverInstallx86_869d103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_869d103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_869d103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_869d103c_02f5;, EventLogService

[DriverServicex86_869d103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 869d103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_869d103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_869d103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_869d103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_869d103c_02f5;, EventLogService

[DriverServicex64_869d103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 869d103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[869d103c_02f5_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00003255
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x28202077  
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f          
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x0000077f          
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x0000077f
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx 29 
[DriverInstallx86_86a0103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86a0103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86a0103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86a0103c;, EventLogService

[DriverServicex86_86a0103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86a0103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86a0103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86a0103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86a0103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86a0103c;, EventLogService

[DriverServicex64_86a0103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86a0103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86a0103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000041a
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x08202077   
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000007df           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000007df 
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80000000
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx 30 
[DriverInstallx86_86a0103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86a0103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86a0103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86a0103c_02f5;, EventLogService

[DriverServicex86_86a0103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86a0103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86a0103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86a0103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86a0103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86a0103c_02f5;, EventLogService

[DriverServicex64_86a0103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86a0103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86a0103c_02f5_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00003055
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x08202077  
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f          
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x0000077f          
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x0000077f 
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx 31
[DriverInstallx86_86a3103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86a3103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86a3103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86a3103c;, EventLogService

[DriverServicex86_86a3103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86a3103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86a3103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86a3103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86a3103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86a3103c;, EventLogService

[DriverServicex64_86a3103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86a3103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86a3103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000041a
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18202077   
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000007bf           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000007bf
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80000000
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx 32 
[DriverInstallx86_86a3103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86a3103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86a3103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86a3103c_02f5;, EventLogService

[DriverServicex86_86a3103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86a3103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86a3103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86a3103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86a3103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86a3103c_02f5;, EventLogService

[DriverServicex64_86a3103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86a3103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86a3103c_02f5_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00003155
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18202077  
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x000007bf          
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x000007bf           
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000007df          
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000007df
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx 33
[DriverInstallx86_86a5103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86a5103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86a5103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86a5103c;, EventLogService

[DriverServicex86_86a5103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86a5103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86a5103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86a5103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86a5103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86a5103c;, EventLogService

[DriverServicex64_86a5103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86a5103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86a5103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000041a
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x28202077   
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x0000077f
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80000000
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx 34
[DriverInstallx86_86a5103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86a5103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86a5103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86a5103c_02f5;, EventLogService

[DriverServicex86_86a5103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86a5103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86a5103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86a5103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86a5103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86a5103c_02f5;, EventLogService

[DriverServicex64_86a5103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86a5103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86a5103c_02f5_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00003255
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x28202077  
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f          
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x0000077f          
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x0000077f
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx 35
[DriverInstallx86_86a8103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86a8103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86a8103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86a8103c;, EventLogService

[DriverServicex86_86a8103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86a8103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86a8103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86a8103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86a8103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86a8103c;, EventLogService

[DriverServicex64_86a8103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86a8103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86a8103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000041a
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x08202077   
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000007df           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000007df 
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80000000
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx 36
[DriverInstallx86_86a8103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86a8103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86a8103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86a8103c_02f5;, EventLogService

[DriverServicex86_86a8103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86a8103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86a8103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86a8103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86a8103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86a8103c_02f5;, EventLogService

[DriverServicex64_86a8103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86a8103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86a8103c_02f5_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00003055
HKR,"sd", "gg_sw_def1", 0x00010001, 0x07000000
HKR,"sd", "gg_sw_def2", 0x00010001, 0x07361022
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400
HKR,"sd", "gg_sw_def5", 0x00010001, 0x02000076
HKR,"sd", "gg_sw_def6", 0x00010001, 0x00025432
HKR,"sd", "gg_sw_def7", 0x00010001, 0x01046076
HKR,"sd", "gg_sw_def8", 0x00010001, 0x62011000
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def12", 0x00010001, 0x10330020
HKR,"sd", "gg_sw_def13", 0x00010001, 0x00020607
HKR,"sd", "gg_sw_def14", 0x00010001, 0x40000000
HKR,"sd", "gg_sw_def15", 0x00010001, 0x12200310
HKR,"sd", "gg_sw_def16", 0x00010001, 0x08202077  
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f          
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x0000077f          
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x0000077f 
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ssc_ctrl", 0x00010001, 0x0000001e
HKR,"sd", "level1_window_num_200m", 0x00010001, 0x00000004
HKR,"sd", "level2_window_num_200m", 0x00010001, 0x00000006
HKR,"sd", "level3_window_num_200m", 0x00010001, 0x00000007
HKR,"sd", "level1_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level2_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "level3_window_num_100m", 0x00010001, 0x0000000b
HKR,"sd", "ssc_cen_200m", 0x00010001, 0x00000088
HKR,"sd", "ssc_max1_200m", 0x00010001, 0x000000A0
HKR,"sd", "ssc_min1_200m", 0x00010001, 0x00000060
HKR,"sd", "ssc_max2_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_min2_200m", 0x00010001, 0x00000050
HKR,"sd", "ssc_bottom_max3_200m", 0x00010001, 0x000000a4
HKR,"sd", "ssc_bottom_min3_200m", 0x00010001, 0x00000040
HKR,"sd", "ssc_top_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_top_min3_200m", 0x00010001, 0x00000010
HKR,"sd", "ssc_history_max3_200m", 0x00010001, 0x000000c0
HKR,"sd", "ssc_history_min3_200m", 0x00010001, 0x00000010


;cfg idx 37
[DriverInstallx86_86bb103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86bb103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86bb103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86bb103c;, EventLogService

[DriverServicex86_86bb103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86bb103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86bb103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86bb103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86bb103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86bb103c;, EventLogService

[DriverServicex64_86bb103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86bb103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86bb103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019

HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000

HKR,"sd", "driver_item", 0x00010001, 0x8000001a

HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711

HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513

HKR,"sd", "gg_sw_def16", 0x00010001, 0x38204077   

HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  

HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  

HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        

HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x000006ff          

HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x000006ff            

HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000003ff           

HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000003ff           

HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a

HKR,"sd", "psd_mode", 0x00010001, 0x80040a01

HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a

HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032

HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000303


;cfg idx 38
[DriverInstallx86_86bb103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86bb103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86bb103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86bb103c_02f5;, EventLogService

[DriverServicex86_86bb103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86bb103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86bb103c_02f5.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86bb103c_02f5.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86bb103c_02f5.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86bb103c_02f5;, EventLogService

[DriverServicex64_86bb103c_02f5]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86bb103c_02f5_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86bb103c_02f5_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019

HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000

HKR,"sd", "driver_item", 0x00010001, 0x8000001a

HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711

HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513

HKR,"sd", "gg_sw_def16", 0x00010001, 0x38204077   

HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  

HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  

HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        

HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x000006ff          

HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x000006ff            

HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000003ff           

HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000003ff           

HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a

HKR,"sd", "psd_mode", 0x00010001, 0x80040a01

HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a

HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000

HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032

HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000303


;cfg idx 39
[DriverInstallx86_86bc103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86bc103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86bc103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86bc103c;, EventLogService

[DriverServicex86_86bc103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86bc103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86bc103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86bc103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86bc103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86bc103c;, EventLogService

[DriverServicex64_86bc103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86bc103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86bc103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019    
HKR,"sd","max_access_mode",0x00010001,0x80000002
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def16", 0x00010001, 0x28204077   
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000003ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000007fe           
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000202


;cfg idx 40
[DriverInstallx86_86bd103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86bd103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86bd103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86bd103c;, EventLogService

[DriverServicex86_86bd103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86bd103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86bd103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86bd103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86bd103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86bd103c;, EventLogService

[DriverServicex64_86bd103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86bd103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86bd103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019    
HKR,"sd","max_access_mode",0x00010001,0x80000002
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def16", 0x00010001, 0x28204077   
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000003ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000007fe           
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000202


;cfg idx 41
[DriverInstallx86_86be103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_86be103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_86be103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_86be103c;, EventLogService

[DriverServicex86_86be103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86be103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_86be103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_86be103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_86be103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_86be103c;, EventLogService

[DriverServicex64_86be103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 86be103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[86be103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019    
HKR,"sd","max_access_mode",0x00010001,0x80000002
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def16", 0x00010001, 0x28204077   
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000003ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000007fe           
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000202   



;cfg idx 42 
[DriverInstallx86_874b103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_874b103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_874b103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_874b103c;, EventLogService

[DriverServicex86_874b103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 874b103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_874b103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_874b103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_874b103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_874b103c;, EventLogService

[DriverServicex64_874b103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 874b103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[874b103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019    
HKR,"sd","max_access_mode",0x00010001,0x80000002
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def16", 0x00010001, 0x28204077   
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000003ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000007fe           
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000202


;cfg idx 43 
[DriverInstallx86_874c103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_874c103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_874c103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_874c103c;, EventLogService

[DriverServicex86_874c103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 874c103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_874c103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_874c103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_874c103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_874c103c;, EventLogService

[DriverServicex64_874c103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 874c103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[874c103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019    
HKR,"sd","max_access_mode",0x00010001,0x80000002
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def16", 0x00010001, 0x28204077   
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000003ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000007fe           
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000202


;cfg idx 44 
[DriverInstallx86_87fb103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_87fb103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_87fb103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_87fb103c;, EventLogService

[DriverServicex86_87fb103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 87fb103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_87fb103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_87fb103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_87fb103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_87fb103c;, EventLogService

[DriverServicex64_87fb103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 87fb103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[87fb103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019    
HKR,"sd","max_access_mode",0x00010001,0x80000002
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def16", 0x00010001, 0x28204077   
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000003ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000007fe           
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000202


;cfg idx 45 
[DriverInstallx86_87fc103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_87fc103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_87fc103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_87fc103c;, EventLogService

[DriverServicex86_87fc103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 87fc103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_87fc103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_87fc103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_87fc103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_87fc103c;, EventLogService

[DriverServicex64_87fc103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 87fc103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[87fc103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000019    
HKR,"sd","max_access_mode",0x00010001,0x80000002
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10057513
HKR,"sd", "gg_sw_def16", 0x00010001, 0x28204077   
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106        
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f            
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000003ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000007fe           
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "ldo_switch_dealy_time_before_clk_on", 0x00010001, 0x00000032
HKR,"sd", "recovery_arg_2", 0x00010001, 0x00050003
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000202

;cfg idx 46 
[DriverInstallx86_856e103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_856e103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_856e103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_856e103c;, EventLogService

[DriverServicex86_856e103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 856e103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_856e103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_856e103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_856e103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_856e103c;, EventLogService

[DriverServicex64_856e103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 856e103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[856e103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000099
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000041a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10037513
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106                          
HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400   
HKR,"sd", "sw_sela_sdr104", 0x00010001, 0x000007ff
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000003ff
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x000007ef
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x000007ef
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000101
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000101

;cfg idx 47 
[DriverInstallx86_882c103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_882c103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_882c103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_882c103c;, EventLogService

[DriverServicex86_882c103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 882c103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_882c103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_882c103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_882c103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_882c103c;, EventLogService

[DriverServicex64_882c103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 882c103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[882c103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000099
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10037513
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18102077   
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f          
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000006ff
 HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000 
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000101

;cfg idx 48 
[DriverInstallx86_882d103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_882d103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_882d103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_882d103c;, EventLogService

[DriverServicex86_882d103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 882d103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[DriverInstallx64_882d103c.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_882d103c.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_882d103c.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_882d103c;, EventLogService

[DriverServicex64_882d103c]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
DelReg         = cfg_DelReg
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 882d103c_cfg
AddReg         = default_cfg_intel
AddReg         = autorun_addreg

[882d103c_cfg]
HKR,"sd", "output_ctrl", 0x00010001, 0x00000099
HKR,"sd", "ssc_ctrl", 0x00010001, 0x00000000
HKR,"sd", "driver_item", 0x00010001, 0x8000001a
HKR,"sd", "gg_sw_def10", 0x00010001, 0x64141711
HKR,"sd", "gg_sw_def11", 0x00010001, 0x10037513
HKR,"sd", "gg_sw_def16", 0x00010001, 0x18102077   
HKR,"sd", "gg_sw_def3", 0x00010001, 0x01015412                  
HKR,"sd", "gg_sw_def4", 0x00010001, 0x01062400  
HKR,"sd", "gg_sw_def9", 0x00010001, 0x70603106
HKR,"sd", "sw_selb_sdr50", 0x00010001, 0x0000077f           
HKR,"sd", "hw_selb_sdr50", 0x00010001, 0x0000077f          
HKR,"sd", "sw_selb_sdr104", 0x00010001, 0x000006ff           
HKR,"sd", "hw_selb_sdr104", 0x00010001, 0x000006ff
 HKR,"sd", "power_wait_time", 0x00010001, 0x003c000a
HKR,"sd", "psd_mode", 0x00010001, 0x80040a01
HKR,"sd", "auto_poweroff_time", 0x00010001, 0x8000000a
HKR,"sd", "sdr104_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr50_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr25_drv_strength", 0x00010001, 0x00000000
HKR,"sd", "sdr12_drv_strength", 0x00010001, 0x00000000 
HKR,"sd", "ggc_ds_item", 0x00010001, 0x00000101


;Common cfg
[Copybhtv5Icon]
bhtv5Icon.dll

[Copybhtv5Icon_WoW64]
bhtv5Icon.dll


[CopySDPA8220]


[CopySDPA8220_WoW64]


[InterruptMgmtValues]
HKR, "Interrupt Management",0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties",0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties",MSISupported,0x00010001,1

[EventLogService]
AddReg = EventLogService_AddReg

[EventLogService_AddReg]
HKR,,EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,   0x00010001, 7

[pnpsafe_pci_addreg]
HKR, "Parameters\PnpInterface", "5", 0x00010001, 0x00000001

[bus_type]
HKR,"Parameters", "BusType", 0x00010001, 0x0000000C

[cfg_DelReg]
HKR, "seabird"
HKR, "seaeagle"
HKR, "fj2"
HKR, "sd"

[default_cfg_se]


[default_cfg_sb]


[default_cfg_fj2]


[default_cfg_intel]


[autorun_addreg] 
HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010008,"SDHC"
HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010008,"SDXC"
HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010008,"SD"
HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010008,"MMC"
;HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010000,"Brother RemovableDisk(U)"

[Strings]
REG_SZ        = 0x00000000
REG_MULTI_SZ  = 0x00010000
REG_EXPAND_SZ = 0x00020000
REG_BINARY    = 0x00000001
REG_DWORD     = 0x00010001
SERVICEROOT   = "System\CurrentControlSet\Services"

BayHubTech          = "BayHubTech"
BHTPCRDR.DeviceDesc = "BayHubTech Integrated SD controller"
BHTPCRDR.DriverDisk = "BayHubTech Integrated SD controller Driver Disk"
BHTPCRDR.sdhci_DeviceDesc = "BayHubTech Integrated SD controller(SDA Compliant Host)"