;
; UHE Serial HID Minidriver Installation
;
[version]
signature="$Windows NT$"
Class=HIDClass
ClassGUID={745a17a0-74d3-11d0-b6fe-00a0c90f57da}
Provider=%V_WIDCOMM%
CatalogFile=uhebthid-x64.cat
DriverVer=12/11/2015,12.0.1.870

[DestinationDirs]
CopyFiles.driver = 12

[SourceDisksNames]
1 = %Source_Description%,,,

[SourceDisksFiles]
uhebthid.sys = 1

[Manufacturer] 
%V_WIDCOMM%=WIDCOMM, NTamd64

[WIDCOMM.NTamd64]
%UHE_HID_DESCRIPTION%=UHE_HID,UHEBTBUS\HID

[UHE_HID.NT]
CopyFiles = CopyFiles.driver
Include=input.inf
Needs=HID_Inst.NT


[UHE_HID.NT.Services]
AddService = uhebthid,0x00000002,uhebthid_Serv_Inst,

[uhebthid_Serv_Inst] 
ServiceType = %SERVICE_KERNEL_DRIVER% 
StartType = %SERVICE_DEMAND_START% 
ErrorControl = %SERVICE_ERROR_IGNORE% 
ServiceBinary = %12%\uhebthid.sys 

[CopyFiles.driver]
uhebthid.sys

[Strings] 
;  *******Localizable Strings******* 
Source_Description="Broadcom Installation Disk #1"
V_WIDCOMM="Broadcom"
UHE_HID_DESCRIPTION= "Bluetooth Serial UHE HID"

SERVICE_BOOT_START = 0x0 
SERVICE_SYSTEM_START = 0x1 
SERVICE_AUTO_START = 0x2 
SERVICE_DEMAND_START = 0x3 
SERVICE_DISABLED = 0x4 

SERVICE_KERNEL_DRIVER = 0x1 
SERVICE_ERROR_IGNORE = 0x0 
SERVICE_ERROR_NORMAL = 0x1 
SERVICE_ERROR_SEVERE = 0x2 
SERVICE_ERROR_CRITICAL = 0x3 

