;
; Installation file (.inf) for the device.
;
; (c) Copyright 2000-2004 GeoVision Inc.
;

[Version]
LayoutFile=Layout.inf, Layout1.inf, Layout2.inf
Signature=$CHICAGO$
Class=DVR-Devices
ClassGUID={4d36e96c-e325-11ce-bfc1-0123456789AB}
Provider=%Msft%

[ClassInstall32]
Addreg=DVR-Devices_Class,AdditionalInfo

[DVR-Devices_Class]
HKR,,,,"DVR-Devices"
HKR,,Icon,,"-5"	

[ControlFlags]
;ExcludeFromSelect=*

[Manufacturer]
%Msft%=Manufact

[Manufact]
%DVR.DeviceDesc%=DeviceSection,PCI\VEN_14F1&DEV_8800&SUBSYS_2BEA2040

[DestinationDirs]
DVR.CopyDrivers=10,system32\drivers

[DeviceSection]
AddReg=     DVR.AddReg,Common.AddReg
CopyFiles=  DVR.CopyDrivers
KnownFiles= DVR.KnownFiles

[DVR.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,GVMP2.sys

[Common.AddReg]
HKLM,%DVR.RegPath%,MpegBufferCount03,0x00010003,1
HKLM,%DVR.RegPath%,MpegBufferCountXP,0x00010003,6
HKLM,%DVR.RegPath%,MpegBufferCount2K,0x00010003,1

[DVR.CopyDrivers]
GVMP2.sys

[DVR.KnownFiles]
GVMP2.sys=safe

[DeviceSection.Services]
AddService = GVMP2,0x00000002,DeviceSection.ServiceInstall


[DeviceSection.ServiceInstall]
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %10%\system32\drivers\gvmp2.sys

[Strings]
Msft				= "GeoVision Inc."

DVR.DeviceDesc		= "GVMP2"
DVR.RegPath="system\currentcontrolset\services\GVMP2"

SERVICE_KERNEL_DRIVER=1
SERVICE_DEMAND_START=3
SERVICE_ERROR_NORMAL=1
