; Gv800.inf
;
; Installation file (.inf) for the Capture device.
;
; (c) Copyright 2001 GeoVision Inc.
;

[Version]
LayoutFile=Layout.inf, Layout1.inf, Layout2.inf
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider=%Msft%

[ControlFlags]
;ExcludeFromSelect=*

[Manufacturer]
%MsftMfg%=Manufact

;------------------------------------------------------------------------------
; These are the files we need installed
;------------------------------------------------------------------------------

[DVR.CopyDrivers]
Gv800.sys

[DVR.KnownFiles]
Gv800.sys=safe

[DestinationDirs]
DVR.CopyDrivers=10,system32\drivers

[Manufact]
%DVR.VideoDeviceDescA%=VideoSection,PCI\VEN_109E&DEV_036E&SUBSYS_40cc45bA
%DVR.AudioDeviceDescA%=AudioSection,PCI\VEN_109E&DEV_0878&SUBSYS_40cc45bA
%DVR.VideoDeviceDescB%=VideoSection,PCI\VEN_109E&DEV_036E&SUBSYS_40cc45bB
%DVR.AudioDeviceDescB%=AudioSection,PCI\VEN_109E&DEV_0878&SUBSYS_40cc45bB
%DVR.VideoDeviceDescC%=VideoSection,PCI\VEN_109E&DEV_036E&SUBSYS_40cc45bC
%DVR.AudioDeviceDescC%=AudioSection,PCI\VEN_109E&DEV_0878&SUBSYS_40cc45bC
%DVR.VideoDeviceDescD%=VideoSection,PCI\VEN_109E&DEV_036E&SUBSYS_40cc45bD
%DVR.AudioDeviceDescD%=AudioSection,PCI\VEN_109E&DEV_0878&SUBSYS_40cc45bD


[DVR.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,Gv800.sys

[VideoSection]
AddReg=     DVR.AddReg
CopyFiles=  DVR.CopyDrivers
KnownFiles= DVR.KnownFiles

[VideoSection.Services]
AddService = Gv800,0x00000002,VideoSection.ServiceInstall

[VideoSection.ServiceInstall]
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %10%\system32\drivers\Gv800.sys

[AudioSection]

[AudioSection.Services]
AddService = , 2  ; null service install

[Strings]
Msft=			"GeoVision Inc."
MsftMfg=		"GeoVision Inc."
DVR.VideoDeviceDescA=	"Gv800 Video Capture #A"
DVR.AudioDeviceDescA=	"Gv800 Audio(NULL) #A"
DVR.VideoDeviceDescB=	"Gv800 Video Capture #B"
DVR.AudioDeviceDescB=	"Gv800 Audio(NULL) #B"
DVR.VideoDeviceDescC=	"Gv800 Video Capture #C"
DVR.AudioDeviceDescC=	"Gv800 Audio(NULL) #C"
DVR.VideoDeviceDescD=	"Gv800 Video Capture #D"
DVR.AudioDeviceDescD=	"Gv800 Audio(NULL) #D"

SERVICE_KERNEL_DRIVER=1
SERVICE_DEMAND_START=3
SERVICE_ERROR_NORMAL=1
