;
; wpdmtp_test.inf
; Media Service Provider driver package for USB-MTP devices.
; Windows 98, Windows ME, Windows 2000, Windows XP
; Copyright (C) 2005, Microsoft Corporation
;
; WARNING: THIS FILE IS PROVIDED FOR TEST PURPOSE ONLY.
;

; ==================== Version section ======================

[Version]
Signature="$CHICAGO$"
Class=WPD
ClassGUID={EEC5AD98-8080-425f-922A-DABF3DE3F69A}
Provider=%Provider%
DriverVer = 08/04/2007, 1.00.0.0

; ==================== Class sections =======================

[ClassInstall32]

; ================= Manufacturer & Models sections ==========

[Manufacturer]
%MfgName%=Test
 
[Test]

; Vendor needs to supply the VID (xxxx) and PID (yyyy)
%Test.DeviceDesc% = Test_MTP, USB\VID_04e8&PID_6702
 

; ================ Win9x Device Install sections ============

[Test_MTP]
Include = wpdmtp.inf
Needs   = WPD.MTP.SW.Registration.9x
 
[Test_MTP.HW]
Include = wpdmtp.inf
Needs   = WPD.MTP.Registration.9x
; Uncomment the following line for a MTP device that does not support PDDRM
; AddReg = MTP.HW.LocalRegistration

; ================= WinNT Device Install sections ===========

[Test_MTP.NT]
 
[Test_MTP.NT.HW]
Include = wpdmtp.inf
Needs   = WPD.MTP.Registration
; Uncomment the following line for a MTP device that does not support PDDRM
; AddReg = MTP.HW.LocalRegistration
 
[Test_MTP.NT.Services]
Include = wpdmtp.inf
Needs   = WPD.MTP.Services

; ================= Device specific registration ============

[MTP.HW.LocalRegistration]
; Create and set this flag to supress queryiug device's storage serial number.  
; This is only needed for a MTP device that does not support PDDRM.
; This flag is set if its value is not 0.
HKR,,"SupressGetStorageSerialNum",0x10001,1
 
; ================= String macro section ====================

[Strings]

; =========== Localizable macro substitutions ===============

Test.DeviceDesc = "SGH-X830"
MfgName         = "SAMSUNG MTP Devices"
Provider        = "SAMSUNG"
